

Keywords:QYB40-165L,Air operated oil pump

Beijing BPM,Beijing Petroleum Machinery Co.,Control System for Surface Mounted BOP Stacks, bop control unit, koomey unit, BPMF BOP CONTROL, accumulator unit, FKDQ1200-9,FKDQ1200-9B,FKDQ960-7,FKDQ640-7,FKQ1440-14,FKQ1200-9,FKQ1280-8,FKQ960-8,FKQ840-8,FKQ800-8,FKQ1280-7,FKQ1200-7,FKQ800-7D,FKQ800-7E,FKQ800-7F,FKQ800-8G,FKQ800-9H,FKQ640-7,FKQ800-6FFKQ720-6,FKQ640-6G,FKQ640-6,FKQ640-6M,FKQ640-6S,FKQ480-5,FKQ480-5C,FKQ480-5E,FKQ480-5B,FKQ480-5D,FKQ320-4B,FKQ3204E,FKQ320-4G,FKQ320-3,FKQ160-4W,FK250-4,FK240-4,FK160-4,FK100-4,FK240-3E,FKQ240-3D,FK240-3,FK125-3,FK125-3B,FK125-2D,FK125-2F,FK50-1

Product name:Air operated oil pump

Model:QYB40-165L





1 Locating sleeve 9163800018 2

2 O-ring seal 5303001010 2 17×2.65

3 Locating sleeve spring 9163800019 2

4 Hexagon fit bolts--Product 4202001820 2 M6×45

5 Standard spring washer 4205030030 2 6

6 Type I hex nut 4204000040 2 M6

7 Steel ball 4371010320 3 16.000

8 Hex bolt 4202000131 4 M8×30

9 Plain washer grade A 4205010040 4 8

10 Standard spring washer 4205030040 5 8

11 Pump head 9165200015 1

12 Gas pipe joint 9163800025 4

13 1/4 pipe plug 9180412000 2

14 Gas pipe gasket seal 9163800024 4

15 Gas pipe nut 9163800023 4

16 Gas pipe 9165200016 2

17 Hex nut 4204000260 1 M8 (DZn）

18 Spool connecting rod and baffle plate 9163800026 1

19 Spool 9163800028 1

20 O-ring seal 9163800043 2 31.2×3.65(聚氨酯)

21 Spool connecting rod 9163800027 1

22 Nut for spool connecting rod 9163800029 1

23 Spool rod 9163800033 1

24 O-ring seal 5303100050 1 85×2.65

25 Seat for pump head 9165200013 1

26 Plain washer grade A 4205010050 20 10

27 Hex bolt 4202001970 10 M10×190(DZn)

28 Parallel pins 4207010080 2 B6×20

29 O-ring seal 5303000950 1 10×2.65

30 Spool sleeve bracket 9163800030 1

31 O-ring seal 5303000160 6 45×2.65

32 Spool sleeve 9165200014 1

33 Pump head plug 9163800016 2

34 Gas baffle 9163800017 2

35 Standard spring washer 4205030050 12 10

36 Type I hex nut – fine thread 4204000150 2 M10×1

37 Piston rod screw cap 9163800031 1

38 Piston gasket 9163800032 1

39 O-ring seal 5303000070 1 22.4×3.55

40 Gasket seal for air cylinder 9165200009 2

41 Piston 9165200012 1

42 O-ring seal 5303101140 1 230×8.6

43 Stop collar for spool rod 9163800035 1

44 Spool rod spring 9163800036 1

45 Spool rod coupling 9163800034 1

46 Piston rod 9163800037 1

47 Air cylinder 9165200023 1

48 O-ring seal 5303001120 1 28×3.55

49 Base 9165200010 1

50 Type I hex nut 4204000060 10 M10

51 Piston rod nut 9163800009 1

52 Piston rod coupling 9165200017 1

53 Connecting rod gasket 9163800039 2

54 Extension rod for base 9165200018 2

55 Plunger rod 9165200007 1

56 Body 9165203000 1

57 Type I hex nut 4204000160 2 M20×1.5

58 Standard spring washer 4205030100 2 20

59 Plain washer grade A 4205010100 2 20

60 Pressure ring 9165202001 1

61 V-fabrics. ring gasket 9165201003 5

62 V-supplement ring gasket 9165201002 4

63 Support ring 9165202002 1

64 Body spring 9165200019 1

65 Spring stop collar 9165200020 1

66 Spring seat 9165200021 1

67 Plunger copper sleeve 9165200006 1

68 Plunger spring 9165200005 1

69 Support ring 9165201004 1

70 Pressure ring 9165201001 1

71 Pressure cap 9165200004 1

72 Plunger type cylinder 9165200003 1

73 Steel ball catch 9165200002 1

74 Steel ball 4371010150 1 25.400

75 Plunger piston coupling 9165200001 1

76 Male and female angle fittings 9180401000 1